**01. A memory address register specifies the address in memory for the next read or write.**

**02. A memory buffer register contains the data to be written into memory or receives the data read from memory.**

**03. The most common classes of interrupts are: program, timer, I/O and hardware failure.**

**04. A(n) timer interrupt is generated by a timer within the processor and allows the operating system to perform certain functions on a regular basis.**

**05. A(n) Input/Output interrupt is generated by an I/O controller to signal normal completion of an operation, request service from the processor, or to signal a variety of error conditions.**

**06. A disabled interrupt simply means that the processor can and will ignore that interrupt request signal.**

**07. The collection of paths connecting the various modules is called the interconnection structure.**

**08. A bus is a communication pathway connecting two or more devices.**

**09. The control lines are used to control the access to and the use of the data and address lines.**

**10. Bus lines can be separated into two generic types: dedicated and multiplexed.**

**11. With asynchronous timing the occurrence of one event on a bus follows and depends on the occurrence of a previous event.**